The Hybrid Pseudo-Spectral (HPS) Code Nic Brummell PARALLEL CODE: INPUT/OUTPUT

All I/O is cached to seperate I/O processors All processors send data to the I/O processors I/O processors receive data and write single file File is sent directly to the mass store. Process is asynchronous Creates only one file, not one file per processor.

Input reads and redistributes data. Can start up on any number of processors.